# This file describes the network interfaces available on your system
# and how to activate them. For more information, see interfaces(5).

# The loopback network interface
auto lo
iface lo inet loopback

# cote N-adm
allow-hotplug enp0s3
iface enp0s3 inet static
	address 192.168.99.100
	netmask 255.255.255.0

# cote N-dmz
allow-hotplug enp0s8
iface enp0s8 inet static
	address 192.168.100.10
	netmask 255.255.255.0
	gateway 192.168.101.100
	up route add -net 192.168.200.0/24 gw 192.168.100.254
	up route add -net 172.16.0.0/24 gw 192.168.100.254

# cote N-lb-f
allow-hotplug enp0s9
iface enp0s9 inet static
	address 192.168.101.100
	netmask 255.255.255.0
